|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | |
| Petroleum Branch  360-1395 Ellice Ave, Winnipeg, MB R3G 3P2  **T** 204-945-6577 **F** 204-945-0586  [www.manitoba.ca](http://www.manitoba.ca) | | | | | | | |
| **WEEKLY WELL ACTIVITY REPORT** | | | | | | | |
|  |  |  | |  |  | |  |
| PETROLEUM INDUSTRY ACTIVITY REPORT | | | | | | | |
| (January 1/19 – January 14/19) | | | | | | | |
|  |  |  |  | | |  |  |
| **DRILLING ACTIVITY** | **To January 14/19** |  | To January 15/18 | | |  | 2018 Total |
|  |  |  |  | | |  |  |
| Drilling Licences Issued | 6 |  | 5 | | |  | 290 |
| Licences Cancelled | 0 |  | 0 | | |  | 13 |
| Vertical Wells Drilled | 1 |  | 0 | | |  | 13 |
| Horizontal Wells Drilled | 11 |  | 16 | | |  | 263 |
| Stratigraphic Test Holes Drilled | 0 |  | 0 | | |  | 0 |
| Wells Drilled - Total | 12 |  | 16 | | |  | 276 |
| No. of Metres Drilled | 23 363 |  | 32 457 | | |  | 586 264 |
| Wells Re-entered | 0 |  | 0 | | |  | 0 |
| Wells Being Drilled | 5 |  | 2 | | |  | 0 |
| No. of Active Rigs | 6 |  | 6 | | |  | 8 |
| Wells Licenced but Not Spudded | 64 |  | 61 | | |  | 74 |
|  |  |  |  | | |  |  |
| Wells Completed as Potential Oil Wells | 11 |  | 16 | | |  | 271 |
| Wells Abandoned Dry | 0 |  | 0 | | |  | 3 |
| Wells Drilled but Not Completed | 0 |  | 0 | | |  | 0 |
| Other Completions | 1 |  | 0 | | |  | 2 |
|  |  |  |  | | |  |  |
| New Wells on Production | 0 |  | 0 | | |  | 85 |
|  |  |  |  | | |  |  |
| **GEOPHYSICAL ACTIVITY** |  |  |  | | |  |  |
|  |  |  |  | | |  |  |
| Geophysical Programs Licenced | 0 |  | 0 | | |  | 3 |
| Licences Cancelled | 0 |  | 0 | | |  | 1 |
| Kilometers Licenced | 0 |  | 0 | | |  | 82 |
| Kilometers Run | 0 |  | 0 | | |  | 638 |
|  |  |  |  | | |  |  |
|  | **2018** |  | **2017** | | |  |  |
| **OIL PRICES (Average)** | $/m3 ($/bbl) |  | $/m3 ($/bbl) | | |  |  |
|  |  |  |  | | |  |  |
| Month of November | 347.77 (55.26) |  | 447.77 (71.15) | | |  |  |
| Month of December | 259.97 (41.31) |  | 440.28 (69.96) | | |  |  |
|  |  |  |  | | |  |  |
| **OIL PRODUCTION (M3)** | **2018** |  | **2017** | | |  |  |
| Month of August | 189 804.4 |  | 193 117.8 | | |  |  |

**WEEKLY WELL ACTIVITY REPORT**

**14 January 2019**

|  |  |
| --- | --- |
| Lic. No.: 4269 | Waskada Unit No. 4 6A-24-1-26 (WPM)  UWI: 1A0.06-24-001-26W1.00  Status: Abandoned Salt Solution Well (ABD P)  Abandoned Producer: 11-Jan-2019 |
| Lic. No.: 8151 | Tundra St. Lazare HZNTL **13-36-16-28** (WPM)  UWI: 100.14-36-016-28W1.00 – Leg #1  **UWI: 100.13-36-016-28W1.02 – Leg #1 Extension Revised**  **UWI: 100.15-36-016-28W1.03 - Leg #2 Revised**  ***Please note changes to UWI’s & Well Name to reflect As Drilled:***  **UWI: 100.13-36-016-28W1.02 – Leg #1 Extension Revised**  **Licenced as 100.14-36… changed to 100.13-36…**  **Well Name changed from 14-36… to 13-36**  **UWI: 100.15-36-016-28W1.03 - Leg #2 Revised**  **Licenced as 100.14-36… changed to 100.15-36…** |
|  |  |
| Lic. No.: 10313 | Birdtail Unit No. 3 HZNTL **A14-29-16-27** (WPM)  UWI: 102.16-30-016-27W1.00 – Leg #1  **UWI: 102.14-29-016-27W1.02 – Leg #1 Extension Revised**  **UWI: 102.14-29-016-27W1.03 – Leg #2 Revised**  ***Please note revised UWI’s & Well Name to reflect As Drilled:***  **UWI: 102.14-29-016-27W1.02 – Leg #1 Extension Revised**  **Licenced as 102.16-30…changed to 102.14-29…**  **Well Name changed from 16-30…to A14-29…** |
|  | **UWI: 102.14-29-016-27W1.03 – Leg #2 Revised**  **Licenced as 102.16-30… changed to 102.14-29** |
| Lic. No.: 11017 | Corex Daly Sinclair Prov. HZNTL **C9-24-9-28** (WPM)  **UWI: 104.09-24-009-28W1.00 Revised**  ***Please note revised UWI and Well Name***  **Licenced as 100.08-24…changed to 104.09-24…**  **Well name changed from 8-24… to C9-24…** |
| Lic. No.: 11055 | North Virden Scallion Unit No. 1 Prov. HZNTL **11-24-11-26** (WPM)  **UWI: 102.11-24-011-26W1.00 – Leg #1 Revised**  UWI: 104.14-24-011-26W1.02 – Leg #2  ***Please note revised UWI & Well Name to reflect As Drilled:***  **102.11-24-011-26W1.00 - Leg #1**  **Licenced as 104.14-24…changed to 102.11-24**  **Well Name changed from A14-24… to 11-24…** |
| Lic. No.: 11059 | Waskada Unit No. 3 HZNTL A14-32-1-25 (WPM)  UWI: 103.14-32-001-25W1.00  Finished Drilling: 08-Jan-2019  Total Depth: 1612.00 m  Intermediate Casing: 139.70 mm @ 1612.00 m with 25.5 t  Rig Released: 08-Jan-2019  Status: Waiting On Service Rig (WOSR)  Waiting On Service Rig: 08-Jan-2019 |
|  |  |
| Lic. No.: 11087 | North Virden Scallion Unit No. 1 HZNTL 6-21-11-26 (WPM)  UWI: 102.06-21-011-26W1.00  Surface Casing: 244.50 mm @ 204.00 m with 12.0 t  Intermediate Casing: 177.80 mm @ 863.00 m with 13.0 t  Finished Drilling: 11-Jan-2019  Total Depth: 1821.00 m  Rig Released: 11-Jan-2019 |
|  | Status: Waiting On Service Rig (WOSR)  Waiting On Service Rig: 11-Jan-2019 |
| Lic. No.: 11090 | Corex Virden HZNTL 1-6-10-25 (WPM)  UWI: 100.01-06-010-25W1.00 – Leg #1  **UWI: 100.08-06-010-25W1.02 - Leg #2 Revised**  ***Please note revised UWI to reflect As Drilled:***  **UWI: 100.08-06-010-25W1.02 - Leg #2 Revised**  **Licenced as 100.01-06… changed to 100.08-06…** |
| Lic. No.: 11113 | Tundra Daly Sinclair SWD 5-6-11-28 (WPM)  UWI: 100.05-06-011-28W1.00  Status: Completing (COMP)  Completing: 12-Jan-2019 |
| Lic. No.: 11114 | North Virden Scallion Unit No. 1 HZNTL 15-9-11-26 (WPM)  UWI: 102.15-09-011-26W1.00  Spud Date: 12-Jan-2019  K.B. Elevation: 461.80 m  Surface Casing: 244.50 mm @ 200.00 m with 12.0 t  Status: Running Casing (CSG)  Running Casing: 14-Jan-2019 |
|  |  |
| Lic. No.: 11115 | South Pierson Unit No. 1 Prov. HZNTL 13-16-2-29 (WPM)  UWI: 103.13-16-002-29W1.00  Finished Drilling: 07-Jan-2019  Total Depth: 1842.00 m  Intermediate Casing: 139.70 mm @ 1842.00 m with 44.6 t  Rig Released: 09-Jan-2019 |
|  | Status: Waiting On Service Rig (WOSR)  Waiting On Service Rig: 09-Jan-2019 |
| Lic. No.: 11119 | South Pierson Unit No. 1 HZNTL A12-8-2-29 (WPM)  UWI: 103.12-08-002-29W1.00  Spud Date: 09-Jan-2019  K.B. Elevation: 481.95 m  Surface Casing: 244.50 mm @ 179.00 m with 13.0 t  Status: Drilling Ahead (DR)  Drilling Ahead: 14-Jan-2019 |
|  |  |
| Lic. No.: 11122 | Corex Virden HZNTL 14-3-12-26 (WPM)  UWI: 100.14-03-012-26W1.00  Status: Completing (COMP)  Completing: 12-Jan-2019 |
| Lic. No.: 11127 | Corval Daly Sinclair HZNTL E16-23-8-28 (WPM)  UWI: 106.16-23-008-28W1.00  Status: Completing (COMP)  Completing: 13-Jan-2019 |
| Lic. No.: 11134 | Tundra Daly Sinclair Prov. HZNTL 13-20-10-28 (WPM)  UWI: 102.13-20-010-28W1.00  Status: Completing (COMP)  Completing: 12-Jan-2019 |
| Lic. No.: 11136 | Tundra Daly Sinclair Prov. HZNTL D5B-36-8-29 (WPM)  UWI: 105.05-36-008-29W1.00  Status: Completing (COMP)  Completing: 08-Jan-2019 |
| Lic. No.: 11138 | Daly Unit No. 3 HZNTL A10-12-10-28 (WPM)  UWI: 104.10-12-010-28W1.00  Spud Date: 09-Jan-2019  K.B. Elevation: 493.84 m  Surface Casing: 244.50 mm @ 270.00 m with 13.0 t |
|  | Status: Drilling Ahead (DR)  Drilling Ahead: 14-Jan-2019 |
| Lic. No.: 11141 | Tundra Daly Sinclair Prov. HZNTL 8-32-9-29 (WPM)  UWI: 102.08-32-009-29W1.00  Status: Completing (COMP)  Completing: 10-Jan-2019 |
| Lic. No.: 11144 | Tundra Daly Sinclair HZNTL B9-28-8-28 (WPM)  UWI: 103.09-28-008-28W1.00  ***Please note revision to Report dated 17-Dec-2018:***  ***Drilling Contractor: Trinidad Drilling Ltd. – Rig #10***  Spud Date: 09-Jan-2019  K.B. Elevation: 499.17 m  Surface Casing: 244.50 mm @ 135.00 m with 7.5 t  Finished Drilling: 12-Jan-2019  Total Depth: 2124.00 m  Intermediate Casing: 139.70 mm @ 2124.00 m with 33.0 t  Rig Released: 13-Jan-2019  Status: Waiting On Service Rig (WOSR)  Waiting On Service Rig: 13-Jan-2019 |
|  |  |
| Lic. No.: 11145 | Tundra Daly Sinclair HZNTL B16-28-8-28 (WPM)  UWI: 103.16-28-008-28W1.00 |
|  | Finished Drilling: 08-Jan-2019  Total Depth: 2126.00 m  Intermediate Casing: 139.70 mm @ 2126.00 m with 33.0 t  Rig Released: 08-Jan-2019  Status: Completing (COMP)  Completing: 14-Jan-2019 |
|  |  |
| Lic. No.: 11150 | Sinclair Unit No. 19 HZNTL C13-25-8-29 (WPM)  UWI: 104.13-25-008-29W1.00  Intermediate Casing: 177.80 mm @ 1062.00 m with 16.0 t  Finished Drilling: 09-Jan-2019  Total Depth: 2475.00 m  Rig Released: 10-Jan-2019 |
|  | Status: Waiting On Service Rig (WOSR)  Waiting On Service Rig: 10-Jan-2019 |
| Lic. No.: 11151 | Tundra Daly Sinclair HZNTL B1-15-9-29 (WPM)  UWI: 103.01-15-009-29W1.00  Status: Completing (COMP)  Completing: 13-Jan-2019 |
| Lic. No.: 11153 | Corex Daly Sinclair HZNTL 8-31-9-28 (WPM)  UWI: 102.08-31-009-28W1.00  Finished Drilling: 07-Jan-2019  Total Depth: 2353.00 m  Intermediate Casing: 139.70 mm @ 2353.00 m with 38.5 t  Rig Released: 08-Jan-2019 |
|  | Status: Waiting On Service Rig (WOSR)  Waiting On Service Rig: 08-Jan-2019 |
| Lic. No.: 11157 | Cromer Unit No. 2 HZNTL B11-13-9-28 (WPM)  UWI: 103.11-13-009-28W1.00  Status: Moving In Rotary Tools (MIRT)  Moving In Rotary Tools: 14-Jan-2019 |
| Lic. No.: 11163 | Waskada Unit No. 22 HZNTL A11-22-1-25 (WPM)  UWI: 102.11-22-001-25W1.00  Spud Date: 09-Jan-2019  K.B. Elevation: 474.94 m  Finished Drilling: 11-Jan-2019  Total Depth: 1684.00 m  Intermediate Casing: 139.70 mm @ 1684.00 m with 26.5 t  Rig Released: 12-Jan-2019  Status: Waiting On Service Rig (WOSR)  Waiting On Service Rig: 12-Jan-2019 |
|  |  |
| Lic. No.: 11168 | Tundra Daly Sinclair HZNTL A12-14-9-29 (WPM)  UWI: 103.12-14-009-29W1.00  Spud Date: 11-Jan-2018  K.B. Elevation: 526.45 m  Surface Casing: 244.50 mm @ 136.00 m with 7.5 t |
|  | Status: Drilling Ahead (DR)  Drilling Ahead: 14-Jan-2019 |
| Lic. No.: 11175 | Waskada Unit No. 19 HZNTL B1-34-1-25 (WPM)  UWI: 104.01-34-001-25W1.00  Spud Date: 12-Jan-2019  K.B. Elevation: 476.28 m  Surface Casing: 219.10 mm @ 135.00 m with 6.0 t  Intermediate Casing: 139.70 mm @ 1682.00 m with 26.5 t  Status: Drilling Ahead (DR)  Drilling Ahead: 14-Jan-2019 |
|  |  |
| Lic. No.: 11180 | Tundra Waskada HZNTL 9-26-1-25 (WPM)  UWI:100.09-26-001-25W1.00  Licence Issued: 14-Jan-2019  Licensee: Tundra Oil & Gas Limited  Mineral Rights: Tundra Oil & Gas Limited  Contractor: Trinidad Drilling Ltd. - Rig# 12  Surface Location: 9B-27-1-25  Co-ords: 644.51 m S of N of Sec 27  203.12 m W of E of Sec 27  Grd Elev: 472.95 m  Proj. TD: 2527.20 m (Triassic)  Field: Daly Sinclair  Classification: Non Confidential Development  Status: Location(LOC) |