|  |
| --- |
|  |
| Petroleum Branch360-1395 Ellice Ave, Winnipeg, MB R3G 3P2**T** 204-945-6577 **F** 204-945-0586[www.manitoba.ca](http://www.manitoba.ca) |
| **WEEKLY WELL ACTIVITY REPORT** |
|  |  |  |  |  |  |
|  PETROLEUM INDUSTRY ACTIVITY REPORT |
|  (January 1/20 – January 6/20) |
|  |  |  |  |  |  |
| **DRILLING ACTIVITY** | **To January 6/20** |  | To January 7/19 |  | 2019 Total |
|  |  |  |  |  |  |
| Drilling Licences Issued | 1 |  | 5 |  | 225 |
| Licences Cancelled | 0 |  | 0 |  | 17 |
| Vertical Wells Drilled | 0 |  | 1 |  | 13 |
| Horizontal Wells Drilled | 3 |  | 3 |  | 208 |
| Stratigraphic Test Holes Drilled | 0 |  | 0 |  | 0 |
| Wells Drilled - Total | 3 |  | 4 |  | 221 |
| No. of Metres Drilled | 8 853 |  | 7 326 |  | 482 956 |
| Wells Re-entered | 0 |  | 0 |  | 0 |
| Wells Being Drilled | 2 |  | 6 |  | 0 |
| No. of Active Rigs | 5 |  | 6 |  | 7 |
| Wells Licenced but Not Spudded | 56 |  | 70 |  | 58 |
|  |  |  |  |  |  |
| Wells Completed as Potential Oil Wells | 2 |  | 3 |  | 216 |
| Wells Abandoned Dry | 0 |  | 0 |  | 1 |
| Wells Drilled but Not Completed | 1 |  | 0 |  | 0 |
| Other Completions | 0 |  | 1 |  | 4 |
|  |  |  |  |  |  |
| New Wells on Production | 0 |  | 0 |  | 2 |
|  |  |  |  |  |  |
| **GEOPHYSICAL ACTIVITY** |  |  |  |  |  |
|  |  |  |  |  |  |
| Geophysical Programs Licenced | 0 |  | 0 |  | 4 |
| Licences Cancelled | 0 |  | 0 |  | 1 |
| Kilometers Licenced  | 0 |  | 0 |  | 580 |
| Kilometers Run | 0 |  | 0 |  | 20 |
|  |  |  |  |  |  |
|  | **2019** |  | **2018** |  |  |
| **OIL PRICES (Average)** | $/m3 ($/bbl) |  | $/m3 ($/bbl) |  |  |
|  |  |  |  |  |  |
| Month of October |  405.35 (64.41) |  |  490.37 (77.92) |  |  |
| Month of November |  443.23 (70.43) |  |  347.77 (55.26) |  |  |
|  |  |  |  |  |  |
| **OIL PRODUCTION (M3)** | **2018** |  | **2017** |  |  |
| Month of August | 189 804.4 |  | 193 117.8 |  |  |

**WEEKLY WELL ACTIVITY REPORT**

**06 January 2020**

|  |  |
| --- | --- |
| Lic. No.: 1536 | Virden Roselea Unit No. 1 WIW 1-36-10-26 (WPM)UWI: 100.01-36-010-26W1.00Status: Water Injection Well (WIW)Water Injection Well: 20-Nov-2019 |
| Lic. No.: 5681 | Routledge Unit No.1 HZNTL WIW 4-22-9-25 (WPM)UWI: 102.04-22-009-25W1.00 Status: Water Injection Well (WIW)Water Injection Well: 14-Nov-2019 |
| Lic. No.: 6267 | Routledge Unit No.1 Prov. HZNTL WIW 11-32-9-25 (WPM)UWI: 102.11-32-009-25W1.00 – Leg #1UWI: 102.11-32-009-25W1.02 – Leg #2Status: Water Injection Well (WIW)Water Injection Well: 30-Oct-2019 |
|  |  |
| Lic. No.: 6904 | Ewart Unit No. 14 HZNTL WIW 9-10-8-28 (WPM)UWI: 100.09-10-008-28W1.00 Status: Water Injection Well (WIW)Water Injection Well: 10-Sep-2019 |
| Lic. No.: 7602 | Ewart Unit No. 14 HZNTL WIW 8-10-8-28 (WPM)UWI: 100.08-10-008-28W1.00 Status: Water Injection Well (WIW)Water Injection Well: 28-Sep-2019 |
| Lic. No.: 7754 | Sinclair Unit No. 19 Prov. HZNTL WIW 4-14-9-29 (WPM)UWI: 100.04-14-009-29W1.00 Status: Water Injection Well (WIW)Water Injection Well: 23-Aug-2019 |
| Lic. No.: 9289 | Ewart Unit No. 13 HZNTL WIW A16-31-8-28 (WPM)UWI: 103.16-31-008-28W1.00 Status: Water Injection Well (WIW)Water Injection Well: 10-Sep-2019 |
| Lic. No.: 10032 | Ewart Unit No. 11 Prov. HZNTL WIW A8-16-8-28 (WPM)UWI: 103.08-16-008-28W1.00 Status: Water Injection Well (WIW)Water Injection Well: 18-Oct-2019 |
| Lic. No.: 10316 | Routledge Unit No. 1 HZNTL WIW 2-32-9-25 (WPM)UWI: 102.02-32-009-25W1.00 Status: Water Injection Well (WIW)Water Injection Well: 31-Oct-2019 |
| Lic. No.: 10888 | East Manson Unit No. 9 HZNTL WIW 15-16-13-28 (WPM)UWI: 100.15-16-013-28W1.00 Status: Water Injection Well (WIW)Water Injection Well: 16-Aug-2019 |
| Lic. No.: 11216 | Tundra Daly Sinclair HZNTL C8-8-10-28 (WPM)UWI: 106.08-08-010-28W1.00 Spud Date: 02-Jan-2020K.B. Elevation: 519.62 mSurface Casing: 244.50 mm @ 137.00 m with 7.8 t |
|  | Status: Drilling Ahead (DR)Drilling Ahead: 06-Jan-2020 |
| Lic. No.: 11267 | Corex Virden HZNTL 1-1-10-26 (WPM)UWI: 102.01-01-010-26W1.00 - Leg #1UWI: 102.01-01-010-26W1.02 - Leg #2**UWI: 102.01-01-010-26W1.00 - Leg #1**Finished Drilling: 05-Jan-2020Total Depth: 2006.00 m**UWI: 102.01-01-010-26W1.02 - Leg #2**Kick-Off Date: 05-Jan-2020Kick-Off Point: 835.00 m |
|  | Status: Drilling Ahead (DR)Drilling Ahead: 06-Jan-2020 |
|  |  |
| Lic. No.: 11333 | South Pierson Unit No. 2 Prov. HZNTL B3-20-2-29 (WPM)UWI: 103.03-20-002-29W1.00 Finished Drilling: 04-Jan-2020Total Depth: 2176.00 mIntermediate Casing: 139.70 mm @ 2176.00 m with 53.1 tRig Released: 06-Jan-2020 |
|  | Status: Waiting On Service Rig (WOSR)Waiting On Service Rig: 06-Jan-2020 |
| Lic. No.: 11334 | South Pierson Unit No. 2 HZNTL A4-19-2-29 (WPM)UWI: 103.04-19-002-29W1.00 ***Please note revision to Report dated 09-Sep-2019:******Drilling Contractor: Stampede Drilling Inc. – Rig #7***Status: Moving In Rotary Tools (MIRT)Moving In Rotary Tools: 06-Jan-2020 |
| Lic. No.: 11368 | Tundra Daly Sinclair HZNTL A8-27-9-29 (WPM)UWI: 103.08-27-009-29W1.00 ***Please note revision to Report dated 02-Dec-2019:******Drilling Contractor: Ensign Drilling Inc. – Rig #12***Spud Date: 03-Jan-2020K.B. Elevation: 535.64 mSurface Casing: 244.50 mm @ 135.00 m with 7.5 tFinished Drilling: 06-Jan-2020Total Depth: 2345.00 m |
|  | Status: Running Casing (CSG)Running Casing: 06-Jan-2020 |
| Lic. No.: 11373 | Tundra Daly Sinclair Prov. HZNTL B5-11-9-29 (WPM)UWI: 103.05-11-009-29W1.00 ***Please note revision to Report dated 23-Dec-2019:******Drilling Contractor: Ensign Drilling Inc. – Rig #9***Spud Date: 03-Jan-2020K.B. Elevation: 527.58 mSurface Casing: 244.50 mm @ 136.00 m with 7.5 tFinished Drilling: 06-Jan-2020Total Depth: 2326.00 mIntermediate Casing: 139.70 mm @ 2326.00 m with 34.25 tRig Released: 06-Jan-2020 |
|  | Status: Waiting On Service Rig (WOSR)Waiting On Service Rig: 06-Jan-2020 |
| Lic. No.: 11395 | Tundra Daly Sinclair HZNTL B8-12-9-29 (WPM)UWI: 103.08-12-009-29W1.00 Status: Moving In Rotary Tools (MIRT)Moving In Rotary Tools: 06-Jan-2020 |
| Lic. No.: 11400 | Sinclair Unit No. 11 HZNTL 3-35-7-29 (WPM)UWI:102.03-35-007-29W1.00Licence Issued: 06-Jan-2020Licensee: Tundra Oil & Gas LimitedMineral Rights: Tundra Oil & Gas LimitedContractor: Ensign Drilling Inc. - Rig# 10Surface Location: 4B-34-7-29Co-ords: 60.00 m N of S of Sec 34 90.00 m E of W of Sec 34Grd Elev: 520.60 mProj. TD: 3183.40 m (Devonian)Field: Daly SinclairClassification: Non Confidential DevelopmentStatus: Location(LOC) |
|  |  |